**2016 WATER QUALITY REPORT – CORRECTION NOTICE**

**LIVONIA WATER SYSTEM**

Public Water Supply ID: LA1077022

The following data for the highest chlorine running average was missed in our previously published 2016 Water Quality Report:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Disinfectant** | **Date** | **Highest Running Annual Average** | **Unit** | **Range** | **MRDL** | **MRDLG** | **Typical Source** |  |
| Chlorine | 2016 | 1.08 | ppm | 0.7 - 2.1 | 4 | 4 | Water additive used  to control microbes |

-MRDL: Maximum residual disinfectant level – The highest level of a disinfectant allowed in drinking water.

-MRDLG: Maximum residual disinfectant level goal – The level of a drinking water disinfectant below which there is no known or expected risk to health.

-ppm: Parts per million or Milligrams per liter (mg/L)

If you have any questions, please contact 225-637-2981.